A blue circle with text and symbols

Description automatically generated

**AMERICAN INTERNATIONAL UNIVERSITY–BANGLADESH (AIUB)**

**FACULTY OF SCIENCE & TECHNOLOGY**

**DEPARTMENT OF ELECTRICAL AND ELECTRONIC ENGINEERING**

**DIGITAL LOGIC AND CIRCUITS LABORATORY**

**FALL 2023-2024**

**Section: Q Group: 2 Exp No: 01**

**LAB REPORT ON**

Studying different digital logic gates and designing basic logic gates using universal gates.

**Supervised By**

**DR. TANBIR IBNE ANOWAR**

**Submitted By:**

|  |  |  |
| --- | --- | --- |
| Name | ID | Contribution |
| TRIDIB SARKAR | **22-46444-1** | Theory research & appendices writing |
| MD. FAHIM MURSHED | **22-46695-1** | Syntax writing, Resource Collecting |
| S.M. MUJAHID SOUROV | **22-49679-3** | Experimental Data, Analysis, Result |
| MD. ATIK ISHRAK SUJON | **22-46684-1** | Procedure, Multisim, MS Word |
| NUSHRAT JAHAN | **22-46149-1** | Discussion writing & Reference collecting |

Date of Submission: **October 19th, 2023**

**TABLE OF CONTENTS**

|  |  |
| --- | --- |
| **TOPICS** | **Page no.** |
| 1. **Cover Page** | 1 |
| 1. **Table of Contents** | 2 |
| **Abstract** | 3 |
| **Theory** | 3 |
| **Apparatus** | 6 |
| **Experimental Procedure** | 6 |
| **Circuit Diagram** | 6 |
| **Images** | 7 |
| **IC Configuration** | 12 |
| **MULTISIM** | 13 |
| **Discussion** | 18 |
| **References** | 18 |

**ABSTRACT:**

In this experiment, we gained knowledge about the characteristics of various logic gates and developed familiarity with digital trainer boards and digital integrated circuits (ICs). We successfully created different gates using universal gates and comprehended logical expressions and the application of universal gates in integrated circuits.

**THEORY:**

**Part I**

**Basic Logic IC’s:**

An integrated circuit, also known as an IC, chip, or microchip, consists of electronic circuits condensed onto a small semiconductor plate called a "chip," typically made of silicon. This allows for a significantly smaller size compared to discrete circuits composed of separate components. The trainer board used in this experiment utilizes various integrated circuits to execute distinct logical operations.

**Methodology:**

In this experiment, we compared Digital signals and analog signals in that they were encoded in binary (0 and 1) format, meaning each bit was represented by two distinct amplitudes.

A black and red line

Description automatically generated with low confidenceCodes were often used to keep the information secret or break it into pieces manageable by technology. Digital signals could be processed by digital circuit components, using less bandwidth and electromagnetic interference. Information storage was easier in digital systems than in analog ones. The noise immunity of digital systems allowed data to be stored and retrieved without degradation. ICs had two main advantages over discrete circuits: cost and performance. A logic gate was an elementary building block of a digital circuit, with two inputs and one output.

|  |  |
| --- | --- |
| **Operation** | **Expression** |
| AND | Y = AB |
| OR | Y = A+B |
| NOT | Y = A' |
| XOR | Y = AB' + A'B |
| NAND | Y= A' + B' |
| NOR | Y= A' B' |

**AND Operation:**

A table with numbers and symbols

Description automatically generatedThe AND operation produces a high if all the inputs are high. Here is the symbol and Truth Table of AND gate.

A black and white symbol

Description automatically generated

**Pin configuration for IC-74HC08N:**

74HC series devices are designed to work with a 5V power supply, allowing voltages from 2V to 5V for most circuits.

**OR Operation:**

The OR operation produces a high output when any of the inputs are high. Here is the symbol and Truth Table of OR gate.

A table with numbers and a few words

Description automatically generated with medium confidenceA black and white drawing of a pointy object

Description automatically generated

**Pin configuration for IC-74HC32N:**

74HC32 is a Quad 2-input OR gate with low current consumption and wide voltage range, with high noise immunity characteristics.

**NOT Operation:**

The NOT operation is implemented by an inverter to change one logic level to another. Here is the symbol and Truth Table of NOT gate.

A symbol of a triangle

Description automatically generatedA table with numbers and symbols

Description automatically generated

**Pin configuration for IC-74HC04N:**

The 74HC04 is a hex inverter with six inverters, clamp diodes, current limiting resistors, and CMOS input level.

**XOR Operation:**

The XOR gate acts like a logical "either/or" gate, with the output being high if either input is high, low if both inputs are low, or 0 if both inputs are the same. Here is the symbol and Truth Table of XOR gate.

A table with numbers and text

Description automatically generated

A black and white symbol

Description automatically generated

**Pin configuration for IC-74HC86N:**

HC86 is a quad 2-input XOR gate with advanced silicon gate CMOS technology, low power consumption and high noise immunity. It has a voltage range of 2V-5V and an input current of 1A.

**Part II:**

**Study of Universal Gates:**

Universal Gates are Logic Gates that can be used to create any Logic Gate, such as NOT, AND, OR, XOR, XNOR, etc. NAND and NOR Gates are examples of Universal Gates.


The objective of this lab is to implement different logic functions using universal gates.

**NAND operation:**

The NAND gate acts as an AND gate followed by a NOT gate, resulting in a high output if both inputs are high. Here is the symbol and Truth Table of NAND gate.

A table with numbers and letters

Description automatically generated



**Pin configuration for IC-74HC00N:**

The device code HC00 is compatible with Standard CMOS outputs, with an operating voltage range of 2.0-5 V and low input current of 1.0 A.

**NOR operation:**

A picture containing text, number, screenshot, font

Description automatically generatedThe NOR gate is a combination OR gate followed by an inverter with a low output if both inputs are low. Here is the symbol and Truth Table of NOR gate.

A picture containing text, sketch, diagram, white

Description automatically generated

**Pin configuration for IC-74HC02N:**

The 74HC02 is a high-speed Si-gate CMOS device with a quadrature 2 -input NOR function and a low input current of 1.0 A.


**Apparatus:**


* Digital trainer board.
* IC or Integrated Circuits (7400,7402,7404,7408,7432,7486)
* Power supply.
* Connecting wires.
* LEDs (green and red)


**Experimental Procedure:**

* Ensured all components needed were ready to use.
* Digital trainer board was set up first and provided with a power source relevant to each of the IC(4V).
* Each IC of different logic gates were chosen to place on the digital trainer board.
* Excluding the 1st and 14th IC connection we tried specific sequences according to the specific logic gates to create logic output.
* One power switch for NOT gate and two switches for other gates were always connected to the IC sequence diagram input.
* One red LED was connected with the IC sequence diagram output. AND green LEDS were connected to the input.
* According to the truth table of different logic gates. Variations were performed.

**Circuit Diagram:   
Implementing AND gate, OR gate & NOT gate using NAND gate:**


****






**Implementing AND gate, OR gate & NOT gate using NOR gate:**

****





**Images:**

A white electronic device with black wires and switches

Description automatically generated **NOT gate:**A white electronic device with black wires and switches

Description automatically generated

A white electronic device with black wires


Description automatically generated**OR gate:**A white electronic device with blue knobs and wires

Description automatically generated


A electronic device with wires and switches

Description automatically generatedA electronic device with wires and switches


Description automatically generated


**AND gate:  
A white electronic device with black wires and switches



Description automatically generatedA circuit board with wires and switches



Description automatically generated**



**NAND gate:  
A white electronic device with black and red buttons and switches

Description automatically generatedA white electronic device with blue knobs and buttons

Description automatically generated**


**NOT gate implementation using NAND gate:  
**

**OR gate implementation using NAND gate:  
**




**AND gate implementation using NAND gate:  
A white electronic device with blue knobs and buttons

Description automatically generatedA white electronic device with blue knobs and black wires


Description automatically generated**

**NOT gate implementation using NOR gate:  
A white electronic device with black wires and buttons


Description automatically generated**

**OR gate implementation using NOR gate:  
A white electronic device with wires and switches

Description automatically generated**

**AND gate implementation using NOR gate:  
A electronic device with wires

Description automatically generated**

**A electronic device with wires and switches

Description automatically generated**

**IC Configuration:**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  | | --- | --- | --- | | 01 | 1A Vcc | 14 | | 02 | 13 | | 1B 4B | | 03 | 12 | | 1Y 4A | | 04 | 11 | | 2A 4Y | | 05 | 10 | | 2B 3B | | 06 | 09 | | 2Y 3A | | 07 | 08 | | GND 3Y | |  |  | |  |  |  | |  |  |  |  | | --- | --- | --- | --- | | 01 | 1Y | Vcc | 14 | | 02 | 13 | | 1A | 4Y | | 03 | 12 | | 1B | 4B | | 04 | 11 | | 2Y | 4A | | 05 | 10 | | 2A | 3Y | | 06 | 09 | | 2B | 3B | | 07 | 08 | | GND 3A | | |  |  | |  |  |  | |  |  |  |  | | --- | --- | --- | --- | | 01 | 1A | Vcc | 14 | | 02 | 13 | | 1Y | 6A | | 03 | 12 | | 2A | 6Y | | 04 | 11 | | 2Y | 5A | | 05 | 10 | | 3A | 5Y | | 06 | 09 | | 3Y | 4A | | 07 | 08 | | GND 4Y | | |  |  | |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  | |  | |  | |
|  | 7400 | |  |  | 7402 | |  |  | 7404 | |  |
| |  |  |  | | --- | --- | --- | | 01 | 1A Vcc | 14 | | 02 | 13 | | 1B 4B | | 03 | 12 | | 1Y 4A | | 04 | 11 | | 2A 4Y | | 05 | 10 | | 2B 3B | | 06 | 09 | | 2Y 3A | | 07 | 08 | | GND 3Y | |  |  | |  |  |  | |  |  |  |  | | --- | --- | --- | --- | | 01 | 1A | Vcc | 14 | | 02 | 13 | | 1B | 4B | | 03 | 12 | | 1Y | 4A | | 04 | 11 | | 2A | 4Y | | 05 | 10 | | 2B | 3B | | 06 | 09 | | 2Y | 3A | | 07 | 08 | | GND 3Y | | |  |  | |  |  |  | |  |  |  |  | | --- | --- | --- | --- | | 01 | 1A | Vcc | 14 | | 02 | 13 | | 1B | 4B | | 03 | 12 | | 1Y | 4A | | 04 | 11 | | 2A | 4Y | | 05 | 10 | | 2B | 3B | | 06 | 09 | | 2Y | 3A | | 07 | 08 | | GND 3Y | | |  |  | |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  | |  | |  | |
|  | 7408 | |  |  | 7432 | |  |  | 7486 | |  |

**MULTISIM:**

**PART I:**

**Simulation for NOT gate:**

**A diagram of a circuit

Description automatically generatedA diagram of a computer

Description automatically generated**

**Simulation for OR gate:**

**A diagram of a computer

Description automatically generatedA diagram of a computer

Description automatically generated**

**A diagram of a computer

Description automatically generatedA diagram of a computer

Description automatically generated**

**Simulation for AND gate:**

A diagram of a circuit

Description automatically generatedA diagram of a circuit

Description automatically generated

A diagram of a circuit

Description automatically generatedA diagram of a circuit

Description automatically generated

**Simulation for NAND gate:**

A diagram of a circuit

Description automatically generatedA diagram of a circuit

Description automatically generated

A diagram of a circuit

Description automatically generatedA diagram of a circuit

Description automatically generated

**Simulation for NOR gate:**

**A diagram of a computer

Description automatically generatedA diagram of a computer

Description automatically generated**

A diagram of a circuit

Description automatically generatedA diagram of a circuit

Description automatically generated

**Simulation for X-OR gate:**

A diagram of a machine

Description automatically generatedA diagram of a space ship

Description automatically generated

A diagram of a computer

Description automatically generatedA diagram of a rocket

Description automatically generated

**PART II:  
Implementing NOT gate using NAND gate:**

A diagram of a circuit

Description automatically generatedA diagram of a circuit

Description automatically generated

**Implementing OR gate using NAND gate:**

A diagram of a circuit

Description automatically generatedA diagram of a circuit

Description automatically generated


A diagram of a circuit

Description automatically generated A diagram of a circuit

Description automatically generated

**Implementing AND gate using NAND gate:**

A diagram of a circuit

Description automatically generated

A diagram of a circuit

Description automatically generatedA diagram of a circuit

Description automatically generated

A diagram of a circuit

Description automatically generatedA diagram of a circuit

Description automatically generated**Implementing XOR gate using NAND gate:**A diagram of a circuit

Description automatically generatedA diagram of a circuit

Description automatically generated

A diagram of a circuit

Description automatically generated**Implementing NOT gate using NOR gate:**

A diagram of a circuit

Description automatically generated

A diagram of a circuit


Description automatically generatedA diagram of a connection

Description automatically generatedA diagram of a circuit

Description automatically generatedA diagram of a diagram

Description automatically generatedA diagram of a connection

Description automatically generated**Implementing OR gate using NOR gate:  
  
Implementing AND gate using NOR gate:**



A diagram of a circuit

Description automatically generatedA diagram of a circuit


Description automatically generated

**Implementing XOR gate using NOR gate:**

A diagram of a circuit

Description automatically generatedA diagram of a circuit

Description automatically generatedA diagram of a circuit

Description automatically generated **Question & Answers:**

**1.What do you mean by universal gate?**

**Ans:** A universal gate refers to a logic gate that can be used to implement any other type of logic gate. In other words, a universal gate has the capability to perform the functions of all other basic logic gates, such as AND, OR, NOT, NAND, NOR, and XOR gates. By using a combination of universal gates, any logical function can be realized.

The two most common universal gates are the NAND gate (NOT-AND) and the NOR gate (NOT-OR). This means that any logical expression or circuit can be constructed using only NAND gates or NOR gates. These gates are considered universal because they can perform all the logical operations required to implement any digital system.

**2.What are the ICs required in this experiment?**

**Ans:** In the first part of the experiment where an X-OR gate is constructed using only NAND gates, the specific ICs required would depend on the number of inputs and outputs desired for the gates. NAND gates can be implemented using various ICs, such as 74LS00, 74HC00, CD4011, or CD4093, among others. These ICs typically contain multiple NAND gates in a single package. We have used 74HC00 in this experiment.

In the second part of the experiment where an X-OR gate is constructed using only NOR gates, again the choice of ICs would depend on the desired number of inputs and outputs. NOR gates can be implemented using ICs like 74LS02, 74HC02, CD4001, or CD4002, among others. These ICs usually contain multiple NOR gates in a single package. We have used 74HC02 in this experiment.

The specific ICs needed may vary based on the trainer board or equipment being used and the availability of different ICs. It's important to refer to the documentation or specifications of the trainer board or consult the experiment guidelines for the recommended ICs to be used in the circuit construction.

**3. Construct a circuit of output F, where F=AB + BC + CA, by using NAND gates only and show the output states for each of the available conditions.**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **A** | **B** | **C** | **F** | **Simulation** |
| **0** | **0** | **0** | **1** |  |
| **0** | **0** | **1** | **1** |  |
| **0** | **1** | **0** | **1** |  |
| **0** | **1** | **1** | **1** |  |
| **1** | **0** | **0** | **1** |  |
| **1** | **0** | **1** | **1** |  |
| **1** | **1** | **0** | **1** |  |
| **1** | **1** | **1** | **0** |  |

**Discussion and Conclusion:**

In this experiment, we have used Multisim software for Simulations. While using this, we faced some problems. Overall, using the software to locate the solution was simple, and a beginner's ability to draw a circuit was average. Firstly, we need to understand truth-table and the design of logic gates. Afterward, we can decide how to prepare for working with Multisim Software. We have successfully and error-free assembled all the components in the breadboard. We have successfully verified that there are no issues in connecting the circuit wires. At last, the Truth-table for the logic gates were verified by the results and simulations and they matched with each other.

**Reference:**

“Digital Fundamentals” by Thomas L. Floyd

* + - [www.tutorialspoint.com](www.tutorialspoint.com%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20)
    - [www.electronics-tutorials.ws](http://www.electronics-tutorials.ws)
    - [www.faculty.kfupm.edu.sa](www.faculty.kfupm.edu.sa%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20%20)